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	PJM 2026 Black Start Reliability Backstop RFP 
Level 1 Proposal Response



RESPONSES DUE: NOVEMBER 20, 2026
PROPOSAL INFORMATION:
	Proposal Type: Choose an item.

	Fuel Assurance Type: Choose an item.

	Resource Status: Choose an item.



GENERAL INFORMATION:
Company Name: _____________________________________________________________________________________________
Unit Name: __________________________________________________________________________________________________
Unit Address: ________________________________________________________________________________________________
Unit ICAP: __________________________________________________________________________________________________
Unit Type: __________________________________________________________________________________________________
Interconnection Voltage Level: __________________________________________________________________________________
Interconnection Switchyard Name: _______________________________________________________________________________
TO Zone (if known): ___________________________________________________________________________________________
Contact Name: _______________________________________________________________________________________________
Contact Address: _____________________________________________________________________________________________
Contact Email: _______________________________________________________________________________________________
Contact Phone: ______________________________________________________________________________________________

FUEL ASSURANCE INFORMATION:  
Fuel Assured Black Start Units must be capable of running 16 hours or more during a restoration event. Fuel assurance is achieved by either:
a. storing at least 16 hours of fuel and non- fuel consumables on site,
b. can operate independently on 2 or more interstate pipelines,
c. being directly connected to a natural gas gathering facility,
d. or having a hydro or non-hydro intermittent or hybrid resource that has been evaluated by the Transmission Provider to be capable of providing no less than 16 hours of operation per day, which need not be continuous, at a megawatt level that provides a confidence level of 90% based on an evaluation of the unit's historical operation over a representative period of time, and meets any other requirements specified in the PJM manuals.


Primary Fuel: __________________________       Secondary Fuel (if applicable): _______________________________
Is a different start-up fuel required for the BS unit for either primary or secondary fuels (e.g ignitor gas, if applicable)?  
YES  ☐ NO ☐     If YES, provide details ______________________________________________________________
For gas fired units (check if applicable):
☐ Single pipeline connection
Provide information on gas contract arrangements (e.g. firm transportation, etc.): ____________________
☐  Can operate independently on 2 or more interstate pipelines
	Provide information on which pipelines: _____________________________________________________
☐ Is directly connected to a natural gas gathering system
For oil fired units, is there oil storage on site (min.16hrs)?               	                 YES ☐  NO ☐
For storage units (battery, pumped storage) can 16hrs of fuel be stored?                 YES ☐  NO ☐
For pumped storage units can 16hrs of fuel be held back for restoration events?     YES ☐  NO ☐
For intermittent or hybrid resources, PJM will evaluate to confirm unit can operate 16 hours per day, which need not be continuous, at a megawatt level that provides a confidence level of 90% based on an evaluation of the unit's historical operation over a representative period of time. 

OPERATIONAL INFORMATION:
Proposed Black Start MWs: _____________________________________________________________________________________
Unit minimum load (under current air permit): _______________________________________________________________________
Emission limitations for operation below minimum (e.g., start-up time to reach air permit compliance): __________________________
Are you willing to obtain a permit modification or waiver to operate at any load during an emergency event?  YES ☐  NO ☐
For Combined Cycle (CC) Units Only
Simple Cycle available:      YES ☐  NO ☐
Steam bypass available.    YES ☐  NO ☐
Percent of CT Output allowed by steam bypass: ______________________________________________________
Duration limit (in # of hours): ______________________________________________________________________

Please send all 2026 Black Start Reliability Backstop RFP Level 1 Responses to BlackStart@pjm.com by November 20, 2026
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